Blinker Codes

00 - Main loop active
01 - Dialup mode
02 - Ethernet - DHCP
03 - Ethernet - DHCP Bad
03 - Ethernet - Static IP

10 - XMIT OK
11 - Couldn't establish connection to server
12 - DNS problem
13 - Exception transmitting logger config
14 - Exception transmitting device configuration
15 - Exception transmitting logger status
16 - Exception transmitting data
17 - Bad XML received from server
18 - Bad response received from server
19 - Bad URL on XMIT

20 - Error opening serial port
21 - No Dial Tone
22 - Phone busy
23 - Timeout in dialup connection
24 - Authorization error
25 - PPP Rejected
26 - No or bad modem response
27 - Other PPP error
